erasing/blank adblue box instruction 
- install usb driver
- take off 4 screws and open box ,  
- put jumper on , to connect 2 pins together 
- plug mini usb cable to board , and other end to computer 
- wait 30-50 seconds , green lamp will  be blinking  , it means that box is erased and ready for programming
- disconnect usb cable

programming
- take jumper off
- connect adblue box to computer by usb cable 
- run truck-adblue-emu v5.exe 
- choose truck model 
- click start 
- yellow lamp should be on  
- disconnect cable  , and fit box to truck  
see instructions 
