- connect the box to laptop ,  (mini usb is on board ) 

- if laptop asks you for drivers , to install hardware ,  drivers are on CD 

- when drivers installed  , disconnect box 

erasinf box procedure : 

- put jumper on (you have 2 pins on board  , just connect them together ) 

- connect to laptop  , wait 4- 50 seconds until green lamp will be  blinking 

- it means box is erased and ready for programming 



programming: 

- make sure thta jumper on board is off  (pins  not connected) 

- connect box to laptop , open truck-adblue-emu v5.exe  

-choose brand of truck and click  start 

- orange lamp should be on  ,

- now box is ready for learning on truck 



- make sure that adblue on truck is working  ,and truck has no errors 

- connect 5 cables , following diagram in instruction 

- turn key on , (orange lamp will be on )  wait 5 seconds when green lapp turn on 

- disconnect adblue , following attached instruction

